Top of Form





Bottom of Form

**Wallpaper symbols**

The following table provides information on the meaning of the standard quality symbols and marks in the wallpaper industry.

|  |  |
| --- | --- |
| **Quality symbols** | |
| http://cdn2.as-creation.com/uploads/RTEmagicC_Lichtbest.sw.jpg.jpg | **good lightfastness** |
| http://www.as-creation.com/uploads/RTEmagicC_scheuerbest.sw_01.jpg.jpg | **scrubbable**  Dirt can be removed with mild soap and water and a soft brush. |
| http://www.as-creation.com/uploads/RTEmagicC_Abwaschb.sw_02.jpg.jpg | **highly resistant to water and washing**  Stains, with the exception of oils and fats, etc. can be cleaned with soapy water and a sponge. |
| http://www.as-creation.com/uploads/RTEmagicC_Abwaschb2.sw_01.jpg.jpg | **resistant to water and washing**  Light stains can be cleaned with a wet sponge. |
| http://www.as-creation.com/uploads/RTEmagicC_geraderansatz.sw_01.jpg.jpg | **straight match approach**  Same patterns are to be hung/arranged at the same height next to each other. |
| http://www.as-creation.com/uploads/RTEmagicC_versetzteransatz.sw_01.jpg.jpg | **offset match approach**  The pattern of the next length must be offset by the specified pattern repeat. |
| http://www.as-creation.com/uploads/RTEmagicC_gestuerzt.sw_01.jpg.jpg | **Reverse alternate lengths**  Every second length is hung upside down. |
| http://www.as-creation.com/uploads/RTEmagicC_Abziehbar.sw_01.jpg.jpg | **completely dry-strippable**  The wallpaper is peeled off at one corner and can then be removed length by length. |
| http://www.as-creation.com/uploads/RTEmagicC_spaltbar.sw_01.jpg.jpg | **peelable**  The top layer of the wallpaper can be peeled off dry. The bottom paper layer remains on the wall as a lining. |
| http://www.as-creation.com/uploads/RTEmagicC_doppeltpraegung_01.jpg.jpg | **form-stable double-embossed wallcovering**  The high quality embossing remains intact during hanging. |
| http://www.as-creation.com/uploads/RTEmagicC_vorgekl.sw_01.jpg.jpg | **pre-paste**The reverse side of the wallpaper has been pre-coated with wallpaper paste and is activated by shortly immersing in water. |