

 ESK RISK ASSESSMENT

|  |  |  |
| --- | --- | --- |
| OPERATION/PROCESSMANUAL HANDLING | DATE: | No**3** |
| LOCATION  |
| EQUIPMENT USED Ladders, step ladders, podiums, paint and materials  | CAN TASK BE ELIMINATED? | Yes | No**X** |
| **RISK PRIOR TO CONTROLS** |
| **HAZARDS IDENTIFIED** | **Low** | **Med** | **High** |
| Sprains & Strains and crushed limbs | **X** |  |  |
| EXPOSED PERSONS  Site operatives | TOTAL NUMBERS AFFECTED  |
| FREQUENCY OF EXPOSURE  Daily/Low | DURATION OF EXPOSURE Low/minimal over an 8 hour working day. |
| CONTROL MEASURES ALREADY IN PLACE1. Operatives are experienced in carrying paint and equipment on a regular basis as part of their daily work and are aware of the dangers of moving and lifting. Maximum lift of 10kgs
2. HSE information on manual handling provided to operative and regular toolbox talks
3. All operatives are told to seek assistance when carrying ladders, stepladders and podiums
 | EXTENT TO WHICH THEY CONTROL RISK1. Operatives are aware of correct lifting techniques.
2. Toolbox talks carried out to reiterate manual handling procedures.
3. To avoid injury to operative.
 |
| ADDITIONAL MEASURES REQUIREDReview for each task as required throughout the contract. Trainees to be supervised | ACTION BYManagement, supervisors & operatives.  | BY WHENPrior to contract start date and on-going throughout contract.  |
| STATEMENT OF RESIDUAL RISKSWhen the detailed control measures in place are adhered to, the risks above should be reduced to an acceptable level.  |
| ADDITIONAL REQUIREMENTS FOR VULNERABLE GROUPS Ensure that physical capabilities are taken into account when allocating works.  |
| MONITORING RESULTSMonitoring is required to ensure that the control remain effective.  |
| ASSESSOR – NAME | POSITIONDirector | REVIEW DATE01.06.21 | LAST REVISED01.06.20 |